|  |  |
| --- | --- |
|  | National University of Technology (NUTECH)  IJP Road, Sector I-12  Islamabad  Telephone : 051-5476805  106/SCM/NUTECH  31 May 2021 |

To: M/s

Subject: Request for Quotation**: - Electrical Lab Tools**

**Please provide quotation for following items. Quotes will be submitted in closed envelop and must reached to SCM Office latest by 03 June 2020 before 1130 hrs.**

|  |  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- | --- |
| **Ser** | | **Item** | **Specifications** | | **A/U** | **Country of Origin** | **Qty Req** | **Price/Unit** | **Total Price** |
|  | | **Mechanical tool set** | A practical kit for motor fitting and complimentary set of most reach for hand tools  Machine-Grade CR40 Alloy Steel, 72 Teeth, 3/8" Drive Ratchet Handle  10 x 1/4" Drive Sockets Metric - 4-4.5-5-5.5-6-6.5-7-8-9-10mm  7 x 3/8" Drive Sockets Metric - 11-12-13-14-15-17-19mm  2 x 3/8" Drive Spark Plug Sockets - 5/8"/16mm, 13/16"/19mm  2 x 3/8" Extension Bars - 3"/76mm, 6"/152mm  3/8" Universal Joint  3/8" to 1/4" Adaptor  3/8" Drive Sliding T-bar.  **OR Equivalent** | | No | Imported | 2 |  |  |
|  | | **Torx set, Philips set** | Torx set, Philips set for special screws | | No | Imported | 5 |  |  |
|  | | **Selector switches** | Selector switches For control circuit 1 way and 2 way | | No | Any | 10 Each |  |  |
|  | | **Component Boxes** | Small plastic boxes for component storage Size (HxW) = (1′ x 1′)  25x racks in each box  (Picture attached in Annex-A) | | No | Any | 5 |  |  |
|  | | **Digital Magger** | **FEATURES**  Double molded plastic housing Large dual display with backlight Test hold function for easy operation Easy to carry testing package Over range Indication Low Battery Indication 1mA test current for Meg Ohm range at rated voltage 200mA short current for continuity range Power source: 1.5V AA size Battery x 6 (included)  Accessories: Manual, test leads and plastic carrying case.  **Specifications:**  Voltage AC: 750  Voltage DC: 1000v  Resistance: 200Ω, 2000Ω  Insulation Resistance: 200MΩ, 2000MΩ  Test Voltage: 250V-200MΩ/500V-200MΩ/1000V-2000MΩ  Continuity Test:  Active Sound Level: ≤ 40Ω, Test current ≤ 200mA  **OR Equivalent** | | No | Imported | 2 |  |  |
|  | | **Anti-static Wrist Band Strap** | POSH Anti-static Wrist Band Strap | | No | Any | 100 |  |  |
|  | | **keypad** | 4x4 matrix keypad | | No | Any | 100 |  |  |
|  |  | |  | **Net Total (Without Taxes)** | | | |  |  |
|  |  | |  | **Total Taxes** | | | |  |  |
|  |  | |  | **Gross Total inclusive of all taxes** | | | |  |  |

1. Please provide unit price of each item, Total price per item, Total price of all items without all applicable taxes and total price with all taxes.
2. Please also mention date of quote, **NTN** and **STRN** number in your quotation.
3. Delivery period will be 5 days from the day of placing order.
4. Rates shall be quoted on free delivery basis at NUTECH Islamabad.
5. Please ensure delivery within stipulated time.
6. Quotes must reach in SCM Office 2nd Floor Admin Block NUTECH Islamabad latest

by 03 June 2021.

7. The same RFQ may also be available on NUTECH Website i.e https://nutech.edu.pk/downloads/procurement/rfqs/

1. **LD will be imposed as per rules**.
2. **Quotes will be opened on 03 June 2021.**
3. **Business will be awarded on package deal basis.**
4. 100% payment will be made after successful completion of the order.

Deputy Assistant Director

Supply Chain Management Office

**Annex-A**

